(module YAAJ_WeAct_BlackPill_SWD_2 (layer F.Cu) (tedit 615F665A)
  (descr "Through hole headers for BluePill module. No SWD breakout. Fancy silkscreen.")
  (tags "module BlluePill Blue Pill header SWD breakout")
  (fp_text reference REF** (at 7.62 -3.81) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "WeAct BlackPill" (at 20.32 24.765 90) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
  (fp_line (start 13.97 49.53) (end 13.97 -1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start 16.51 49.53) (end 13.97 49.53) (layer F.SilkS) (width 0.12))
  (fp_line (start 16.51 -1.27) (end 16.51 49.53) (layer F.SilkS) (width 0.12))
  (fp_line (start 13.97 -1.27) (end 16.51 -1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.33 49.59) (end -1.33 1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.33 49.59) (end -1.33 49.59) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.33 1.27) (end 1.33 49.59) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start 13.44 45.72) (end 13.44 50.06) (layer F.CrtYd) (width 0.05))
  (fp_line (start 13.44 -1.8) (end 13.44 45.72) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.8 45.72) (end 1.8 50.06) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.8 -1.8) (end 1.8 45.72) (layer F.CrtYd) (width 0.05))
  (fp_line (start 17.04 50.06) (end 13.44 50.06) (layer F.CrtYd) (width 0.05))
  (fp_line (start 17.04 -1.8) (end 17.04 50.06) (layer F.CrtYd) (width 0.05))
  (fp_line (start 13.44 -1.8) (end 17.04 -1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.8 50.06) (end 1.8 50.06) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.8 -1.8) (end -1.8 50.06) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.93 50.88) (end -3.93 -2.62) (layer F.CrtYd) (width 0.05))
  (fp_line (start 19.17 50.88) (end -3.93 50.88) (layer F.CrtYd) (width 0.05))
  (fp_line (start 19.17 -2.62) (end 19.17 50.88) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.93 -2.62) (end 19.17 -2.62) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.68 -2.37) (end 18.92 -2.37) (layer F.Fab) (width 0.12))
  (fp_line (start -3.68 50.63) (end -3.68 -2.32) (layer F.Fab) (width 0.12))
  (fp_line (start -3.68 50.63) (end 18.92 50.63) (layer F.Fab) (width 0.12))
  (fp_line (start 18.92 -2.37) (end 18.92 50.63) (layer F.Fab) (width 0.12))
  (fp_line (start -3.755 50.705) (end -3.755 -2.445) (layer F.SilkS) (width 0.12))
  (fp_line (start 18.995 50.705) (end -3.755 50.705) (layer F.SilkS) (width 0.12))
  (fp_line (start 18.995 -2.445) (end 18.995 50.705) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.755 -2.445) (end 18.995 -2.445) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.72 3.48) (end 11.52 3.48) (layer F.Fab) (width 0.1))
  (fp_line (start 3.72 3.48) (end 3.72 -2.32) (layer F.Fab) (width 0.1))
  (fp_line (start 11.52 3.48) (end 11.52 -2.32) (layer F.Fab) (width 0.1))
  (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
  (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
  (fp_line (start 1.27 -1.27) (end 1.27 49.53) (layer F.Fab) (width 0.1))
  (fp_line (start 1.27 49.53) (end -1.27 49.53) (layer F.Fab) (width 0.1))
  (fp_line (start -1.27 49.53) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
  (fp_line (start 13.97 -1.27) (end 16.51 -1.27) (layer F.Fab) (width 0.1))
  (fp_line (start 16.51 -1.27) (end 16.51 49.53) (layer F.Fab) (width 0.1))
  (fp_line (start 16.51 49.53) (end 13.97 49.53) (layer F.Fab) (width 0.1))
  (fp_line (start 13.97 49.53) (end 13.97 -1.27) (layer F.Fab) (width 0.1))
  (fp_text user REF** (at 7.62 24.13 90) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user Y@@J (at 2.921 -1.016 90 unlocked) (layer Dwgs.User)
    (effects (font (size 0.5 0.5) (thickness 0.1)))
  )
  (fp_line (start 2.542 43.179) (end 12.702 43.179) (layer F.Fab) (width 0.1))
  (fp_line (start 12.702 43.179) (end 12.702 45.719) (layer F.Fab) (width 0.1))
  (fp_line (start 12.702 45.719) (end 2.542 45.719) (layer F.Fab) (width 0.1))
  (fp_line (start 2.542 45.719) (end 2.542 43.179) (layer F.Fab) (width 0.1))
  (fp_line (start 12.762 43.119) (end 2.482 43.119) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.482 45.779) (end 12.762 45.779) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.762 45.779) (end 12.762 43.119) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.482 43.119) (end 2.482 45.779) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.012 46.249) (end 2.012 42.649) (layer F.CrtYd) (width 0.05))
  (fp_line (start 13.232 46.249) (end 2.012 46.249) (layer F.CrtYd) (width 0.05))
  (fp_line (start 13.232 42.649) (end 13.232 46.249) (layer F.CrtYd) (width 0.05))
  (fp_line (start 13.232 42.649) (end 2.012 42.649) (layer F.CrtYd) (width 0.05))
  (pad 40 thru_hole circle (at 15.24 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 39 thru_hole circle (at 15.24 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 38 thru_hole circle (at 15.24 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 37 thru_hole circle (at 15.24 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 36 thru_hole circle (at 15.24 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 35 thru_hole circle (at 15.24 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 34 thru_hole circle (at 15.24 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 33 thru_hole circle (at 15.24 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 32 thru_hole circle (at 15.24 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 31 thru_hole circle (at 15.24 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 30 thru_hole circle (at 15.24 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 29 thru_hole circle (at 15.24 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 12 thru_hole circle (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 28 thru_hole circle (at 15.24 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 13 thru_hole circle (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 27 thru_hole circle (at 15.24 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 14 thru_hole circle (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 26 thru_hole circle (at 15.24 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 15 thru_hole circle (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 25 thru_hole circle (at 15.24 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 16 thru_hole circle (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 24 thru_hole circle (at 15.24 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 17 thru_hole circle (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 23 thru_hole circle (at 15.24 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 18 thru_hole circle (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 22 thru_hole circle (at 15.24 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 19 thru_hole circle (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 21 thru_hole circle (at 15.24 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 20 thru_hole circle (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 42 thru_hole circle (at 8.892 44.449) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 43 thru_hole circle (at 6.352 44.449) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 41 thru_hole circle (at 11.432 44.449) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 44 thru_hole circle (at 3.812 44.449) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (model D:/Users/admin/Documents/KiCad/Libraries/packages3d/Modules/STM32_Blue_Pill/YAAJ_BluePill_PinHeaders_H_SWD_cp.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model D:/Users/admin/Documents/KiCad/Libraries/packages3d/Modules/STM32_Blue_Pill/YAAJ_BluePill_PinHeaders_No_SWD_cp.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model D:/Users/admin/Documents/KiCad/Libraries/packages3d/Modules/STM32_Blue_Pill/YAAJ_BluePill_PinHeaders_V_SWD_cp.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model D:/Users/admin/Documents/KiCad/Libraries/packages3d/Modules/STM32_Blue_Pill/YAAJ_BluePill_PinSockets_H_SWD_cp.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model D:/Users/admin/Documents/KiCad/Libraries/packages3d/Modules/STM32_Blue_Pill/YAAJ_BluePill_PinSockets_No_SWD_cp.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model D:/Users/admin/Documents/KiCad/Libraries/packages3d/Modules/STM32_Blue_Pill/YAAJ_BluePill_PinSockets_V_SWD_cp.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
