(module "R_0402" (layer F.Cu) (tedit 5DB0AAA5)
  (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
  (tags "resistor 0402")
  (attr smd)
  (fp_text reference "REF**" (at 0 -1.35) (layer F.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)))
  )
  (fp_text value "R_0402" (at 0 1.45) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "%R" (at 2.413 0) (layer F.Fab)
    (effects (font (size 0.7 0.7) (thickness 0.15)))
  )
  (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.1))
  (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.1))
  (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.1))
  (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.1))
  (fp_line (start 0.762 -0.53) (end -0.762 -0.53) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.762 0.53) (end 0.762 0.53) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.8 -0.45) (end 0.8 -0.45) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.8 -0.45) (end -0.8 0.45) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.8 0.45) (end 0.8 -0.45) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.8 0.45) (end -0.8 0.45) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.762 -0.53) (end 0.762 0.53) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.762 -0.53) (end -0.762 0.53) (layer F.SilkS) (width 0.12))
  (pad "2" smd rect (at 0.45 0) (size 0.4 0.6) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "1" smd rect (at -0.45 0) (size 0.4 0.6) (layers "F.Cu" "F.Paste" "F.Mask"))
  (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
