(module HHKB_JP_HRS_DF14_15P (layer F.Cu) (tedit 59086BE9)
  (descr http://www.mouser.com/ds/2/185/e53800017-12550.pdf)
  (tags "HHKB JP, HRS, Hirose, DF14, 15P")
  (fp_text reference CN1 (at 9.3 -3) (layer F.SilkS) hide
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text value JP (at 8.75 -2.1) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (pad "" np_thru_hole circle (at 20.1 -1.1) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -2.6 -1.1) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
  (pad 17 smd rect (at 19.9 -5.1) (size 2 2.6) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 10 0) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 11.25 0) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 13.75 0) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 12.5 0) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 17.5 0) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 16.25 0) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 15 0) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 5 0) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 6.25 0) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 8.75 0) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 7.5 0) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 2.5 0) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 3.75 0) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at 1.25 0) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at 0 0) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at -2.4 -5.1) (size 2 2.6) (layers F.Cu F.Paste F.Mask))
)
