(module Kailh_socket_PG1350 (layer F.Cu) (tedit 5DD50E5C)
  (descr "Kailh \"Choc\" PG1350 keyswitch socket mount")
  (tags kailh,choc)
  (attr smd)
  (fp_text reference REF** (at -5 -2) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_text value Kailh_socket_PG1350 (at 0 8.255) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.6 -3.1) (end 2.6 -3.1) (layer Eco2.User) (width 0.15))
  (fp_line (start 2.6 -3.1) (end 2.6 -6.3) (layer Eco2.User) (width 0.15))
  (fp_line (start 2.6 -6.3) (end -2.6 -6.3) (layer Eco2.User) (width 0.15))
  (fp_line (start -2.6 -3.1) (end -2.6 -6.3) (layer Eco2.User) (width 0.15))
  (fp_line (start -7 -6) (end -7 -7) (layer F.SilkS) (width 0.15))
  (fp_line (start -7 7) (end -6 7) (layer F.SilkS) (width 0.15))
  (fp_line (start -6 -7) (end -7 -7) (layer F.SilkS) (width 0.15))
  (fp_line (start -7 7) (end -7 6) (layer F.SilkS) (width 0.15))
  (fp_line (start 7 6) (end 7 7) (layer F.SilkS) (width 0.15))
  (fp_line (start 7 7) (end 6 7) (layer F.SilkS) (width 0.15))
  (fp_line (start 6 7) (end 7 7) (layer F.SilkS) (width 0.15))
  (fp_line (start 7 -7) (end 7 -6) (layer F.SilkS) (width 0.15))
  (fp_line (start -6.9 6.9) (end 6.9 6.9) (layer Eco2.User) (width 0.15))
  (fp_line (start 6.9 -6.9) (end -6.9 -6.9) (layer Eco2.User) (width 0.15))
  (fp_line (start 6.9 -6.9) (end 6.9 6.9) (layer Eco2.User) (width 0.15))
  (fp_line (start -6.9 6.9) (end -6.9 -6.9) (layer Eco2.User) (width 0.15))
  (fp_line (start -7.5 -7.5) (end 7.5 -7.5) (layer F.Fab) (width 0.15))
  (fp_line (start 7.5 -7.5) (end 7.5 7.5) (layer F.Fab) (width 0.15))
  (fp_line (start 7.5 7.5) (end -7.5 7.5) (layer F.Fab) (width 0.15))
  (fp_line (start -7.5 7.5) (end -7.5 -7.5) (layer F.Fab) (width 0.15))
  (fp_line (start -7 5.6) (end -7 6.2) (layer B.SilkS) (width 0.15))
  (fp_line (start 1.5 3.7) (end -1 3.7) (layer B.SilkS) (width 0.15))
  (fp_arc (start -1 2.2) (end -2.5 2.2) (angle -90) (layer B.SilkS) (width 0.15))
  (fp_line (start -1.5 8.2) (end -2 7.7) (layer B.SilkS) (width 0.15))
  (fp_line (start -2 6.7) (end -2 7.7) (layer B.SilkS) (width 0.15))
  (fp_line (start -7 6.2) (end -2.5 6.2) (layer B.SilkS) (width 0.15))
  (fp_line (start 2 4.2) (end 1.5 3.7) (layer B.SilkS) (width 0.15))
  (fp_line (start 2 7.7) (end 1.5 8.2) (layer B.SilkS) (width 0.15))
  (fp_line (start 1.5 8.2) (end -1.5 8.2) (layer B.SilkS) (width 0.15))
  (fp_arc (start -2.5 6.7) (end -2 6.7) (angle -90) (layer B.SilkS) (width 0.15))
  (fp_line (start -2.5 2.2) (end -2.5 1.5) (layer B.SilkS) (width 0.15))
  (fp_line (start -2.5 1.5) (end -7 1.5) (layer B.SilkS) (width 0.15))
  (fp_line (start -7 1.5) (end -7 2) (layer B.SilkS) (width 0.15))
  (fp_line (start 7 -7) (end 6 -7) (layer F.SilkS) (width 0.15))
  (fp_text user %V (at -1 9) (layer B.Fab)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_text user %R (at -3 5) (layer B.Fab)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_arc (start -2.5 6.7) (end -2 6.7) (angle -90) (layer B.Fab) (width 0.15))
  (fp_line (start 1.5 8.2) (end -1.5 8.2) (layer B.Fab) (width 0.15))
  (fp_line (start 2 7.7) (end 1.5 8.2) (layer B.Fab) (width 0.15))
  (fp_line (start 1.5 3.7) (end -1 3.7) (layer B.Fab) (width 0.15))
  (fp_line (start 2 4.2) (end 1.5 3.7) (layer B.Fab) (width 0.15))
  (fp_line (start -7 6.2) (end -2.5 6.2) (layer B.Fab) (width 0.15))
  (fp_line (start -2 6.7) (end -2 7.7) (layer B.Fab) (width 0.15))
  (fp_line (start -1.5 8.2) (end -2 7.7) (layer B.Fab) (width 0.15))
  (fp_arc (start -1 2.2) (end -2.5 2.2) (angle -90) (layer B.Fab) (width 0.15))
  (fp_line (start -2.5 1.5) (end -7 1.5) (layer B.Fab) (width 0.15))
  (fp_line (start -2.5 2.2) (end -2.5 1.5) (layer B.Fab) (width 0.15))
  (fp_line (start 2 4.25) (end 2 7.7) (layer B.Fab) (width 0.12))
  (fp_line (start -7 1.5) (end -7 6.2) (layer B.Fab) (width 0.12))
  (fp_line (start -7 5) (end -9.5 5) (layer B.Fab) (width 0.12))
  (fp_line (start -9.5 5) (end -9.5 2.5) (layer B.Fab) (width 0.12))
  (fp_line (start -9.5 2.5) (end -7 2.5) (layer B.Fab) (width 0.12))
  (fp_line (start 2 4.75) (end 4.5 4.75) (layer B.Fab) (width 0.12))
  (fp_line (start 4.5 4.75) (end 4.5 7.25) (layer B.Fab) (width 0.12))
  (fp_line (start 4.5 7.25) (end 2 7.25) (layer B.Fab) (width 0.12))
  (pad "" np_thru_hole circle (at 5.22 -4.2) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 2 smd rect (at -8.275 3.75) (size 2.6 2.6) (layers B.Cu B.Paste B.Mask))
  (pad "" np_thru_hole circle (at 0 5.95) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 0 0) (size 3.429 3.429) (drill 3.429) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -5 3.75) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  (pad 1 smd rect (at 3.275 5.95) (size 2.6 2.6) (layers B.Cu B.Paste B.Mask))
  (pad "" np_thru_hole circle (at 5.5 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -5.5 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
)
