(module "TRRS-PJ-320A" (layer F.Cu) (tedit 5D54377F)
  (fp_text reference "REF**" (at 0 14.2) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "TRRS-PJ-320A" (at 0 -5.6) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "Ring2" (at 0 3.25) (layer F.Fab)
    (effects (font (size 0.7 0.7) (thickness 0.1)))
  )
  (fp_text user "Ring1" (at 0 6.25) (layer F.Fab)
    (effects (font (size 0.7 0.7) (thickness 0.1)))
  )
  (fp_text user "Tip" (at 0 10) (layer F.Fab)
    (effects (font (size 0.7 0.7) (thickness 0.1)))
  )
  (fp_text user "Sleeve" (at 0.25 11.4) (layer F.Fab)
    (effects (font (size 0.7 0.7) (thickness 0.1)))
  )
  (fp_line (start 3.05 0) (end -3.05 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.05 12.1) (end -3.05 12.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.05 0) (end 3.05 12.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.05 0) (end -3.05 12.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.8 0) (end 2.8 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.8 0) (end -2.8 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.8 -2) (end -2.8 -2) (layer F.SilkS) (width 0.15))
  (pad "1" thru_hole oval (at -2.3 11.3) (size 1.6 2) (drill oval 0.9 1.3) (layers *.Cu *.Mask))
  (pad "2" thru_hole oval (at 2.3 10.2) (size 1.6 2) (drill oval 0.9 1.3) (layers *.Cu *.Mask))
  (pad "4" thru_hole oval (at 2.3 3.2) (size 1.6 2) (drill oval 0.9 1.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 0 8.6) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 0 1.6) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
  (pad "3" thru_hole oval (at 2.3 6.2) (size 1.6 2) (drill oval 0.9 1.3) (layers *.Cu *.Mask))
  (model "/Users/danny/syncproj/kicad-libs/footprints/Keebio-Parts.pretty/3dmodels/PJ-320A.step"
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 180))
  )
)
