(module "RGB_3528_Blue_Notch" (layer F.Cu) (tedit 5DE3E2DC)
  (descr "RGB LED 3.2x2.7mm http://www.avagotech.com/docs/AV02-0610EN")
  (tags "LED 3227")
  (attr smd)
  (fp_text reference "REF**" (at 0 2.5) (layer F.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)))
  )
  (fp_text value "RGB_BRAG" (at 0 -2.5) (layer F.Fab)
    (effects (font (size 0.7 0.7) (thickness 0.15)))
  )
  (fp_circle (center 2.5 -1.5) (end 2.6 -1.3) (layer F.SilkS) (width 0.15))
  (fp_line (start 2 1.8) (end -2 1.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 2 -1.8) (end 2 1.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -2 -1.8) (end 2 -1.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -2 1.8) (end -2 -1.8) (layer F.SilkS) (width 0.15))
  (fp_text user "G" (at -4.2 0.75) (layer F.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)))
  )
  (fp_text user "R" (at -4.2 -0.75) (layer F.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)))
  )
  (fp_text user "+" (at 4.2 0.75) (layer F.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)))
  )
  (fp_text user "B" (at 4.2 -0.75) (layer F.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)))
  )
  (fp_line (start 0.7 1.4) (end 0.7 -1.4) (layer Cmts.User) (width 0.12))
  (fp_line (start 1.2 -1.4) (end 1.2 1.4) (layer Cmts.User) (width 0.12))
  (fp_line (start 1.2 -1.4) (end -1.6 -1.4) (layer Cmts.User) (width 0.12))
  (fp_line (start 1.6 -1) (end 1.2 -1.4) (layer Cmts.User) (width 0.12))
  (fp_line (start 1.6 1.4) (end 1.6 -1) (layer Cmts.User) (width 0.12))
  (fp_line (start -1.6 1.4) (end 1.6 1.4) (layer Cmts.User) (width 0.12))
  (fp_line (start -1.6 -1.4) (end -1.6 1.4) (layer Cmts.User) (width 0.12))
  (fp_line (start -3.7 1.65) (end -3.7 -1.65) (layer B.CrtYd) (width 0.05))
  (fp_line (start 3.7 1.65) (end -3.7 1.65) (layer B.CrtYd) (width 0.05))
  (fp_line (start 3.7 -1.65) (end 3.7 1.65) (layer B.CrtYd) (width 0.05))
  (fp_line (start -3.7 -1.65) (end 3.7 -1.65) (layer B.CrtYd) (width 0.05))
  (fp_line (start -1.8 1.6) (end -1.8 -1.6) (layer Edge.Cuts) (width 0.15))
  (fp_line (start 1.8 1.6) (end 1.8 -1.6) (layer Edge.Cuts) (width 0.15))
  (fp_line (start -1.8 1.6) (end 1.8 1.6) (layer Edge.Cuts) (width 0.15))
  (fp_line (start -1.8 -1.6) (end 1.8 -1.6) (layer Edge.Cuts) (width 0.15))
  (pad "1" smd rect (at 2.6 -0.75) (size 2 0.7) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at 2.6 0.75) (size 2 0.7) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at -2.6 0.75) (size 2 0.7) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -2.6 -0.75) (size 2 0.7) (layers "F.Cu" "F.Paste" "F.Mask"))
)
