(module TRRS_Jumper (layer F.Cu) (tedit 594F3245)
  (fp_text reference REF** (at 0 4) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value TRRS_Jumper (at 0 -4.25) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4.5 2) (end -4.5 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.5 -2) (end 4.5 2) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.5 -2) (end -4.5 2) (layer B.SilkS) (width 0.15))
  (fp_line (start 4.5 -2) (end 4.5 2) (layer B.SilkS) (width 0.15))
  (fp_line (start -4.5 -2) (end 4.5 -2) (layer B.SilkS) (width 0.15))
  (fp_line (start 4.5 2) (end -4.5 2) (layer B.SilkS) (width 0.15))
  (fp_line (start -4.5 2) (end 4.5 2) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.5 -2) (end -4.5 -2) (layer F.SilkS) (width 0.15))
  (fp_text user VCC (at -6.5 0.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user GND (at 6.5 0.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user GND (at -6.5 0.5) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_text user VCC (at 6.5 0.5) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (pad 4 smd rect (at 3 0.5) (size 1.524 0.762) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -3 0.5) (size 1.524 0.762) (layers B.Cu B.Paste B.Mask))
  (pad 6 smd rect (at 3 0.5) (size 1.524 0.762) (layers B.Cu B.Paste B.Mask))
  (pad 5 thru_hole rect (at 3 -0.5) (size 1.524 0.762) (drill 0.3) (layers *.Cu *.Mask))
  (pad 1 smd rect (at -3 0.5) (size 1.524 0.762) (layers F.Cu F.Paste F.Mask))
  (pad 2 thru_hole rect (at -3 -0.5) (size 1.524 0.762) (drill 0.3) (layers *.Cu *.Mask))
)
