From bfd5f6628a69d8704a84b30c4027149fe1b21efa Mon Sep 17 00:00:00 2001
From: Nicholas Chin <nic.c3.14@gmail.com>
Date: Wed, 30 Oct 2024 20:55:25 -0600
Subject: [PATCH 25/48] mb/dell/optiplex_780: Add USFF variant

Change-Id: I3aa21c743749f4a11a2501f4c121316bd2f1a103
Signed-off-by: Nicholas Chin <nic.c3.14@gmail.com>
---
 src/mainboard/dell/optiplex_780/Kconfig       |   5 +
 src/mainboard/dell/optiplex_780/Kconfig.name  |   3 +
 .../optiplex_780/variants/780_usff/data.vbt   | Bin 0 -> 1917 bytes
 .../variants/780_usff/early_init.c            |   9 +
 .../optiplex_780/variants/780_usff/gpio.c     | 166 ++++++++++++++++++
 .../optiplex_780/variants/780_usff/hda_verb.c |  26 +++
 .../variants/780_usff/overridetree.cb         |  10 ++
 7 files changed, 219 insertions(+)
 create mode 100644 src/mainboard/dell/optiplex_780/variants/780_usff/data.vbt
 create mode 100644 src/mainboard/dell/optiplex_780/variants/780_usff/early_init.c
 create mode 100644 src/mainboard/dell/optiplex_780/variants/780_usff/gpio.c
 create mode 100644 src/mainboard/dell/optiplex_780/variants/780_usff/hda_verb.c
 create mode 100644 src/mainboard/dell/optiplex_780/variants/780_usff/overridetree.cb

diff --git a/src/mainboard/dell/optiplex_780/Kconfig b/src/mainboard/dell/optiplex_780/Kconfig
index 2d06c75c9a..fc649e35d5 100644
--- a/src/mainboard/dell/optiplex_780/Kconfig
+++ b/src/mainboard/dell/optiplex_780/Kconfig
@@ -20,6 +20,9 @@ config BOARD_DELL_OPTIPLEX_780_COMMON
 config BOARD_DELL_OPTIPLEX_780_MT
 	select BOARD_DELL_OPTIPLEX_780_COMMON
 
+config BOARD_DELL_OPTIPLEX_780_USFF
+	select BOARD_DELL_OPTIPLEX_780_COMMON
+
 if BOARD_DELL_OPTIPLEX_780_COMMON
 
 config VGA_BIOS_ID
@@ -30,11 +33,13 @@ config MAINBOARD_DIR
 
 config MAINBOARD_PART_NUMBER
 	default "OptiPlex 780 MT" if BOARD_DELL_OPTIPLEX_780_MT
+	default "OptiPlex 780 USFF" if BOARD_DELL_OPTIPLEX_780_USFF
 
 config OVERRIDE_DEVICETREE
 	default "variants/\$(CONFIG_VARIANT_DIR)/overridetree.cb"
 
 config VARIANT_DIR
 	default "780_mt" if BOARD_DELL_OPTIPLEX_780_MT
+	default "780_usff" if BOARD_DELL_OPTIPLEX_780_USFF
 
 endif # BOARD_DELL_OPTIPLEX_780_COMMON
diff --git a/src/mainboard/dell/optiplex_780/Kconfig.name b/src/mainboard/dell/optiplex_780/Kconfig.name
index db7f2e8fe3..bc84c82a79 100644
--- a/src/mainboard/dell/optiplex_780/Kconfig.name
+++ b/src/mainboard/dell/optiplex_780/Kconfig.name
@@ -2,3 +2,6 @@
 
 config BOARD_DELL_OPTIPLEX_780_MT
 	bool "OptiPlex 780 MT"
+
+config BOARD_DELL_OPTIPLEX_780_USFF
+	bool "OptiPlex 780 USFF"
diff --git a/src/mainboard/dell/optiplex_780/variants/780_usff/data.vbt b/src/mainboard/dell/optiplex_780/variants/780_usff/data.vbt
new file mode 100644
index 0000000000000000000000000000000000000000..dbd764f285ed18f7ee9c54bc777560138bd9b5f7
GIT binary patch
literal 1917
zcmd6nO>7%Q6vzLwGv3{}j$^l`v7@w1q*9sEq+2(b3K>`@c5#TSx@i<uQKf!)+gO;|
zveT#>P+W+B10OwbsGtX=N(gc4jSGjKDkP+yIUo^nsel8$^ny^9H?td8Ra=EiCEn=G
z@6DV4?!2AdojnUv^Rirgvs$heXUkGs9S+{Jc2WPhP0buTak^BTFP@&N9-E$(UtuSX
zS{r`=b+EX|Ig`2a*^5oDdG>8jE-1BBxs`*jgrf_sj_fP;%L|PwURRcCFBMCroNRQv
zmp$2TUhc}qJMB(u#jDG@x6(N85thC4%Z=8hiN}lj&zb2~``u3C;?lCrPQOTnInFqB
zhvdwqWv?lxTb=fVEH;~RPHDPw&g*&|s$pU<Iv53Rb6YTgMPOY8;~P1Yglh^6Fgt1^
zCTz|SVPcSpZ44F@&oNPUMO@&BE3y(57YP_Y!4SZhE?GXYa7k+b0(X|s7u3GDRf^1#
zOd2ZCCPO|I&sHEt;p8UshhHtYQ>7!7x2m<d`Gu2<r+Qc4|6pwd8&zFboH_W7XE7uU
zWW-@Cim&mdY2!O{JANR)OTJG2z>LBtAF!g>K`zPnkx!DpPHuk6{_zc*0qi7)Aet$T
z1ks@8hWS#+6cI5)j1oD86{5PX8Zu2(^OC6M`<pE+J?KFZ=&_JVP1YL=#z<-Q*24K4
zn+$YxrHNJJc`k?_8N=Kres26_#E8GLn2{jfW5P%ge`kL(Btkt=>xo)V)Ow=U6P12c
z=U0uNC9T9v{)-|#h(mSX*hSA8)ZeocL7l4J&!{RSO{6~oTtyn535j!RQh#GA*wTF8
zvasRbO~d!?*FbM3K`W?lHx=v*(jiARIhWyh4^io|;n?@1H>uqJy>0sjV-Dt)_=%bE
zgNO3D@uE5m+7aqi?Y8b+inye%Z=HUmgBtaZ3Lc%OLt+bo+)5BjVwT<{mxT`nde$vb
zV99s{>`r76L#Hr6XW6r|<iq#4Jr?XsxKyeJKEj7;e4SZ^1B12u&iV_9M0*Kem@fmn
z1C>>HT47I`**Q#Vu0QW!^VP-9S{xXzpq_zS#9k-;aXz?b+S!Ne$Kkk6dq<Gj{q2D(
z>&Hj-x+kx1W-4#E&beDT*S)=&NoSE?<-w!G@~aW()0ZN4O&=Q+nZa)p%Vd$k-_$a=
T#w3FFBiyj<XAh$hb(enud`r7S

literal 0
HcmV?d00001

diff --git a/src/mainboard/dell/optiplex_780/variants/780_usff/early_init.c b/src/mainboard/dell/optiplex_780/variants/780_usff/early_init.c
new file mode 100644
index 0000000000..2a55fc3a6e
--- /dev/null
+++ b/src/mainboard/dell/optiplex_780/variants/780_usff/early_init.c
@@ -0,0 +1,9 @@
+/* SPDX-License-Identifier: GPL-2.0-or-later */
+
+#include <northbridge/intel/x4x/x4x.h>
+
+void mb_get_spd_map(u8 spd_map[4])
+{
+	spd_map[0] = 0x50;
+	spd_map[2] = 0x52;
+}
diff --git a/src/mainboard/dell/optiplex_780/variants/780_usff/gpio.c b/src/mainboard/dell/optiplex_780/variants/780_usff/gpio.c
new file mode 100644
index 0000000000..389f4077d7
--- /dev/null
+++ b/src/mainboard/dell/optiplex_780/variants/780_usff/gpio.c
@@ -0,0 +1,166 @@
+/* SPDX-License-Identifier: GPL-2.0-only */
+
+#include <southbridge/intel/common/gpio.h>
+
+static const struct pch_gpio_set1 pch_gpio_set1_mode = {
+	.gpio0  = GPIO_MODE_NATIVE,
+	.gpio1  = GPIO_MODE_NATIVE,
+	.gpio2  = GPIO_MODE_GPIO,
+	.gpio3  = GPIO_MODE_GPIO,
+	.gpio4  = GPIO_MODE_GPIO,
+	.gpio5  = GPIO_MODE_GPIO,
+	.gpio6  = GPIO_MODE_GPIO,
+	.gpio7  = GPIO_MODE_NATIVE,
+	.gpio8  = GPIO_MODE_NATIVE,
+	.gpio9  = GPIO_MODE_GPIO,
+	.gpio10 = GPIO_MODE_GPIO,
+	.gpio11 = GPIO_MODE_NATIVE,
+	.gpio12 = GPIO_MODE_NATIVE,
+	.gpio13 = GPIO_MODE_GPIO,
+	.gpio14 = GPIO_MODE_GPIO,
+	.gpio15 = GPIO_MODE_NATIVE,
+	.gpio16 = GPIO_MODE_GPIO,
+	.gpio17 = GPIO_MODE_NATIVE,
+	.gpio18 = GPIO_MODE_GPIO,
+	.gpio19 = GPIO_MODE_GPIO,
+	.gpio20 = GPIO_MODE_GPIO,
+	.gpio21 = GPIO_MODE_GPIO,
+	.gpio22 = GPIO_MODE_GPIO,
+	.gpio23 = GPIO_MODE_NATIVE,
+	.gpio24 = GPIO_MODE_GPIO,
+	.gpio25 = GPIO_MODE_NATIVE,
+	.gpio26 = GPIO_MODE_NATIVE,
+	.gpio27 = GPIO_MODE_GPIO,
+	.gpio28 = GPIO_MODE_GPIO,
+	.gpio29 = GPIO_MODE_GPIO,
+	.gpio30 = GPIO_MODE_GPIO,
+	.gpio31 = GPIO_MODE_GPIO,
+};
+
+static const struct pch_gpio_set1 pch_gpio_set1_direction = {
+	.gpio2  = GPIO_DIR_INPUT,
+	.gpio3  = GPIO_DIR_INPUT,
+	.gpio4  = GPIO_DIR_INPUT,
+	.gpio5  = GPIO_DIR_INPUT,
+	.gpio6  = GPIO_DIR_INPUT,
+	.gpio9  = GPIO_DIR_OUTPUT,
+	.gpio10 = GPIO_DIR_INPUT,
+	.gpio13 = GPIO_DIR_INPUT,
+	.gpio14 = GPIO_DIR_INPUT,
+	.gpio16 = GPIO_DIR_INPUT,
+	.gpio18 = GPIO_DIR_OUTPUT,
+	.gpio19 = GPIO_DIR_INPUT,
+	.gpio20 = GPIO_DIR_OUTPUT,
+	.gpio21 = GPIO_DIR_INPUT,
+	.gpio22 = GPIO_DIR_INPUT,
+	.gpio24 = GPIO_DIR_INPUT,
+	.gpio27 = GPIO_DIR_INPUT,
+	.gpio28 = GPIO_DIR_OUTPUT,
+	.gpio29 = GPIO_DIR_INPUT,
+	.gpio30 = GPIO_DIR_INPUT,
+	.gpio31 = GPIO_DIR_INPUT,
+};
+
+static const struct pch_gpio_set1 pch_gpio_set1_level = {
+	.gpio9  = GPIO_LEVEL_HIGH,
+	.gpio18 = GPIO_LEVEL_HIGH,
+	.gpio20 = GPIO_LEVEL_HIGH,
+	.gpio28 = GPIO_LEVEL_HIGH,
+};
+
+static const struct pch_gpio_set1 pch_gpio_set1_blink = {
+};
+
+static const struct pch_gpio_set1 pch_gpio_set1_invert = {
+	.gpio13 = GPIO_INVERT,
+};
+
+static const struct pch_gpio_set2 pch_gpio_set2_mode = {
+	.gpio32 = GPIO_MODE_GPIO,
+	.gpio33 = GPIO_MODE_GPIO,
+	.gpio34 = GPIO_MODE_GPIO,
+	.gpio35 = GPIO_MODE_GPIO,
+	.gpio36 = GPIO_MODE_GPIO,
+	.gpio37 = GPIO_MODE_GPIO,
+	.gpio38 = GPIO_MODE_GPIO,
+	.gpio39 = GPIO_MODE_GPIO,
+	.gpio40 = GPIO_MODE_NATIVE,
+	.gpio41 = GPIO_MODE_NATIVE,
+	.gpio42 = GPIO_MODE_NATIVE,
+	.gpio43 = GPIO_MODE_NATIVE,
+	.gpio44 = GPIO_MODE_NATIVE,
+	.gpio45 = GPIO_MODE_NATIVE,
+	.gpio46 = GPIO_MODE_NATIVE,
+	.gpio47 = GPIO_MODE_NATIVE,
+	.gpio48 = GPIO_MODE_GPIO,
+	.gpio49 = GPIO_MODE_GPIO,
+	.gpio50 = GPIO_MODE_NATIVE,
+	.gpio51 = GPIO_MODE_NATIVE,
+	.gpio52 = GPIO_MODE_NATIVE,
+	.gpio53 = GPIO_MODE_NATIVE,
+	.gpio54 = GPIO_MODE_GPIO,
+	.gpio55 = GPIO_MODE_NATIVE,
+	.gpio56 = GPIO_MODE_GPIO,
+	.gpio57 = GPIO_MODE_GPIO,
+	.gpio58 = GPIO_MODE_NATIVE,
+	.gpio59 = GPIO_MODE_NATIVE,
+	.gpio60 = GPIO_MODE_GPIO,
+	.gpio61 = GPIO_MODE_NATIVE,
+	.gpio62 = GPIO_MODE_NATIVE,
+	.gpio63 = GPIO_MODE_NATIVE,
+};
+
+static const struct pch_gpio_set2 pch_gpio_set2_direction = {
+	.gpio32 = GPIO_DIR_INPUT,
+	.gpio33 = GPIO_DIR_INPUT,
+	.gpio34 = GPIO_DIR_INPUT,
+	.gpio35 = GPIO_DIR_OUTPUT,
+	.gpio36 = GPIO_DIR_INPUT,
+	.gpio37 = GPIO_DIR_INPUT,
+	.gpio38 = GPIO_DIR_INPUT,
+	.gpio39 = GPIO_DIR_INPUT,
+	.gpio48 = GPIO_DIR_INPUT,
+	.gpio49 = GPIO_DIR_OUTPUT,
+	.gpio54 = GPIO_DIR_INPUT,
+	.gpio56 = GPIO_DIR_OUTPUT,
+	.gpio57 = GPIO_DIR_INPUT,
+	.gpio60 = GPIO_DIR_OUTPUT,
+};
+
+static const struct pch_gpio_set2 pch_gpio_set2_level = {
+	.gpio35 = GPIO_LEVEL_LOW,
+	.gpio49 = GPIO_LEVEL_HIGH,
+	.gpio56 = GPIO_LEVEL_HIGH,
+	.gpio60 = GPIO_LEVEL_LOW,
+};
+
+static const struct pch_gpio_set3 pch_gpio_set3_mode = {
+	.gpio72 = GPIO_MODE_GPIO,
+};
+
+static const struct pch_gpio_set3 pch_gpio_set3_direction = {
+	.gpio72 = GPIO_DIR_INPUT,
+};
+
+static const struct pch_gpio_set3 pch_gpio_set3_level = {
+};
+
+const struct pch_gpio_map mainboard_gpio_map = {
+	.set1 = {
+		.mode      = &pch_gpio_set1_mode,
+		.direction = &pch_gpio_set1_direction,
+		.level     = &pch_gpio_set1_level,
+		.blink     = &pch_gpio_set1_blink,
+		.invert    = &pch_gpio_set1_invert,
+	},
+	.set2 = {
+		.mode      = &pch_gpio_set2_mode,
+		.direction = &pch_gpio_set2_direction,
+		.level     = &pch_gpio_set2_level,
+	},
+	.set3 = {
+		.mode      = &pch_gpio_set3_mode,
+		.direction = &pch_gpio_set3_direction,
+		.level     = &pch_gpio_set3_level,
+	},
+};
diff --git a/src/mainboard/dell/optiplex_780/variants/780_usff/hda_verb.c b/src/mainboard/dell/optiplex_780/variants/780_usff/hda_verb.c
new file mode 100644
index 0000000000..c94e06b156
--- /dev/null
+++ b/src/mainboard/dell/optiplex_780/variants/780_usff/hda_verb.c
@@ -0,0 +1,26 @@
+/* SPDX-License-Identifier: GPL-2.0-or-later */
+
+#include <device/azalia_device.h>
+
+const u32 cim_verb_data[] = {
+	/* coreboot specific header */
+	0x11d4194a, /* Analog Devices AD1984A */
+	0x10280420, /*  Subsystem ID */
+	10,         /* Number of entries */
+
+	/* Pin Widget Verb Table */
+	AZALIA_PIN_CFG(0, 0x11, 0x02214040),
+	AZALIA_PIN_CFG(0, 0x12, 0x01014010),
+	AZALIA_PIN_CFG(0, 0x13, 0x991301f0),
+	AZALIA_PIN_CFG(0, 0x14, 0x02a19020),
+	AZALIA_PIN_CFG(0, 0x15, 0x01813030),
+	AZALIA_PIN_CFG(0, 0x16, 0x413301f0),
+	AZALIA_PIN_CFG(0, 0x17, 0x41a601f0),
+	AZALIA_PIN_CFG(0, 0x1a, 0x41f301f0),
+	AZALIA_PIN_CFG(0, 0x1b, 0x414501f0),
+	AZALIA_PIN_CFG(0, 0x1c, 0x413301f0),
+};
+
+const u32 pc_beep_verbs[0] = {};
+
+AZALIA_ARRAY_SIZES;
diff --git a/src/mainboard/dell/optiplex_780/variants/780_usff/overridetree.cb b/src/mainboard/dell/optiplex_780/variants/780_usff/overridetree.cb
new file mode 100644
index 0000000000..555b1c1f5c
--- /dev/null
+++ b/src/mainboard/dell/optiplex_780/variants/780_usff/overridetree.cb
@@ -0,0 +1,10 @@
+## SPDX-License-Identifier: GPL-2.0-or-later
+
+chip northbridge/intel/x4x
+	device domain 0 on
+		chip southbridge/intel/i82801jx
+			device pci 1c.0 on  end		# PCIe 1
+			device pci 1c.1 on  end		# PCIe 2
+		end
+	end
+end
-- 
2.47.3

