(module SW_TACT_TH_HORIZ (layer F.Cu) (tedit 59087171)
  (descr http://www.alps.com/products/WebObjects/catalog.woa/E/HTML/Tact/SnapIn/SKHH/SKHHLMA010.html)
  (tags "ALPS SKHH tactile switch")
  (fp_text reference SW1 (at 0.05 -5) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SW_PUSH (at 0 -2.55) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 3.75 2.55) (end 3.75 -1.05) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.75 2.55) (end 3.75 2.55) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.75 -1.05) (end -3.75 2.55) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.75 -4) (end 3.75 -4) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.5 3.85) (end 1.5 2.75) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.5 3.85) (end 1.5 3.85) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.5 2.75) (end -1.5 3.85) (layer F.SilkS) (width 0.15))
  (pad 4 thru_hole circle (at -3.5 -2.5) (size 2 2) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole circle (at 3.5 -2.5) (size 2 2) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at -2.25 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS))
  (pad 1 thru_hole circle (at 2.25 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS))
)
