(module "Elite-C-castellated-29pin" (layer F.Cu) (tedit 5E2CA197)
  (fp_text reference "U1" (at 0 1.625) (layer F.SilkS) hide
    (effects (font (size 1.2 1.2) (thickness 0.2032)))
  )
  (fp_text value "Elite-C-castellated-29pin" (at 0 0) (layer F.SilkS) hide
    (effects (font (size 1.2 1.2) (thickness 0.2032)))
  )
  (fp_text user "D2" (at -11.43 6.35 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "D0" (at -1.27 6.35 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "D1" (at -3.81 6.35 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "GND" (at -6.35 6.35 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "GND" (at -8.89 6.35 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "D4" (at 1.27 6.35 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "C6" (at 3.81 6.35 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "D7" (at 6.35 6.35 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "E6" (at 8.89 6.35 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "B4" (at 11.43 6.35 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "B5" (at 13.589 6.35 90) (layer B.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "B2" (at 11.43 -6.35 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "B3" (at 8.89 -6.35 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "B1" (at 6.35 -6.35 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "F7" (at 3.81 -6.35 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "F6" (at 1.27 -6.35 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "F5" (at -1.27 -6.35 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "F4" (at -3.81 -6.35 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "VCC" (at -6.35 -6.35 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "GND" (at -11.43 -6.35 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "B0" (at -13.97 -6.35 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "B0" (at -13.97 -6.35 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "GND" (at -11.43 -6.35 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "ST" (at -8.92 -6.62212 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "VCC" (at -6.35 -6.35 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "F4" (at -3.81 -6.35 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "F5" (at -1.27 -6.35 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "F6" (at 1.27 -6.35 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "F7" (at 3.81 -6.35 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "B1" (at 6.35 -6.35 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "B3" (at 8.89 -6.35 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "B2" (at 11.43 -6.35 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "B5" (at 13.589 6.35 90) (layer F.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)))
  )
  (fp_text user "B4" (at 11.43 6.35 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "E6" (at 8.89 6.35 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "D7" (at 6.35 6.35 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "C6" (at 3.81 6.35 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "D4" (at 1.27 6.35 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "GND" (at -8.89 6.35 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "GND" (at -6.35 6.35 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "D1" (at -3.81 6.35 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "D0" (at -1.27 6.35 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "D2" (at -11.43 6.35 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "TX0/D3" (at -13.97 4.841872 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "TX0/D3" (at -13.97 4.841872 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_line (start -15.24 8.89) (end 15.24 8.89) (layer F.SilkS) (width 0.381))
  (fp_line (start 15.24 8.89) (end 15.24 -8.89) (layer F.SilkS) (width 0.381))
  (fp_line (start 15.24 -8.89) (end -15.24 -8.89) (layer F.SilkS) (width 0.381))
  (fp_poly (pts (xy -9.36064 -5.820568) (xy -9.06064 -5.820568) (xy -9.06064 -5.720568) (xy -9.36064 -5.720568)) (layer F.SilkS) (width 0.15))
  (fp_poly (pts (xy -8.96064 -5.620568) (xy -8.86064 -5.620568) (xy -8.86064 -5.520568) (xy -8.96064 -5.520568)) (layer F.SilkS) (width 0.15))
  (fp_poly (pts (xy -9.36064 -5.820568) (xy -9.26064 -5.820568) (xy -9.26064 -5.320568) (xy -9.36064 -5.320568)) (layer F.SilkS) (width 0.15))
  (fp_poly (pts (xy -9.36064 -5.420568) (xy -8.56064 -5.420568) (xy -8.56064 -5.320568) (xy -9.36064 -5.320568)) (layer F.SilkS) (width 0.15))
  (fp_poly (pts (xy -8.76064 -5.820568) (xy -8.56064 -5.820568) (xy -8.56064 -5.720568) (xy -8.76064 -5.720568)) (layer F.SilkS) (width 0.15))
  (fp_text user "ST" (at -8.91 -5.929 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_poly (pts (xy -8.95097 -6.933635) (xy -8.85097 -6.933635) (xy -8.85097 -7.033635) (xy -8.95097 -7.033635)) (layer B.SilkS) (width 0.15))
  (fp_poly (pts (xy -9.35097 -7.133635) (xy -8.55097 -7.133635) (xy -8.55097 -7.233635) (xy -9.35097 -7.233635)) (layer B.SilkS) (width 0.15))
  (fp_poly (pts (xy -8.75097 -6.733635) (xy -8.55097 -6.733635) (xy -8.55097 -6.833635) (xy -8.75097 -6.833635)) (layer B.SilkS) (width 0.15))
  (fp_poly (pts (xy -9.35097 -6.733635) (xy -9.05097 -6.733635) (xy -9.05097 -6.833635) (xy -9.35097 -6.833635)) (layer B.SilkS) (width 0.15))
  (fp_poly (pts (xy -9.35097 -6.733635) (xy -9.25097 -6.733635) (xy -9.25097 -7.233635) (xy -9.35097 -7.233635)) (layer B.SilkS) (width 0.15))
  (fp_line (start 15.24 -8.89) (end -17.78 -8.89) (layer B.SilkS) (width 0.381))
  (fp_line (start 15.24 8.89) (end 15.24 -8.89) (layer B.SilkS) (width 0.381))
  (fp_line (start -17.78 8.89) (end 15.24 8.89) (layer B.SilkS) (width 0.381))
  (fp_line (start -17.78 -8.89) (end -17.78 8.89) (layer B.SilkS) (width 0.381))
  (fp_line (start -15.24 -8.89) (end -17.78 -8.89) (layer F.SilkS) (width 0.381))
  (fp_line (start -17.78 -8.89) (end -17.78 8.89) (layer F.SilkS) (width 0.381))
  (fp_line (start -17.78 8.89) (end -15.24 8.89) (layer F.SilkS) (width 0.381))
  (fp_line (start -14.224 -3.556) (end -14.224 3.81) (layer Dwgs.User) (width 0.2))
  (fp_line (start -14.224 3.81) (end -19.304 3.81) (layer Dwgs.User) (width 0.2))
  (fp_line (start -19.304 3.81) (end -19.304 -3.556) (layer Dwgs.User) (width 0.2))
  (fp_line (start -19.304 -3.556) (end -14.224 -3.556) (layer Dwgs.User) (width 0.2))
  (fp_text user "B7" (at 13.362 4.754 90) (layer F.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)))
  )
  (fp_text user "B7" (at 13.362 4.754 90) (layer B.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "F0" (at 13.362 -4.754 90) (layer B.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "F0" (at 13.362 -4.754 90) (layer F.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)))
  )
  (fp_text user "B6" (at 13.462 -6.4 90 unlocked) (layer F.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)))
  )
  (fp_text user "B6" (at 13.462 -6.4 90 unlocked) (layer B.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "C7" (at 13.289 0 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "C7" (at 13.289 0 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "F1" (at 13.289 -2.54 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user "F1" (at 13.289 -2.54 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "D5" (at 13.289 2.54 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user "D5" (at 13.289 2.54 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (pad "1" smd rect (at -13.97 9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -11.43 9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -8.89 9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at -6.35 9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at -3.81 9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at -1.27 9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at 1.27 9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at 3.81 9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "9" smd rect (at 6.35 9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "10" smd rect (at 8.89 9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "11" smd rect (at 11.43 9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "12" smd rect (at 13.97 9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "13" smd rect (at 13.97 -9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "14" smd rect (at 11.43 -9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "15" smd rect (at 8.89 -9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "16" smd rect (at 6.35 -9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "17" smd rect (at 3.81 -9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "18" smd rect (at 1.27 -9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "19" smd rect (at -1.27 -9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "20" smd rect (at -3.81 -9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "21" smd rect (at -6.35 -9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "22" smd rect (at -8.89 -9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "23" smd rect (at -11.43 -9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "24" smd rect (at -13.97 -9.398) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "25" smd rect (at 15.875 5.08 90) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "26" smd rect (at 15.875 2.54 90) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "27" smd rect (at 15.875 0 90) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "28" smd rect (at 15.875 -2.54 90) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "29" smd rect (at 15.875 -5.08 90) (size 2 3.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (model "/Users/danny/Documents/proj/custom-keyboard/kicad-libs/3d_models/ArduinoProMicro.wrl"
    (offset (xyz -13.96999979019165 -7.619999885559082 -5.841999912261963))
    (scale (xyz 0.395 0.395 0.395))
    (rotate (xyz 90 180 180))
  )
)
