From f692cd96a4484b8e60bd112454d1bdbc3c689017 Mon Sep 17 00:00:00 2001
From: Leah Rowe <leah@libreboot.org>
Date: Sun, 5 Nov 2023 11:41:41 +0000
Subject: [PATCH 09/48] dell/e6430: use ME Soft Temporary Disable

i overlooked this. it's set on other boards.

we use me_cleaner anyway, and we set the hap bit, but
this additional setting takes effect even if the ME
region is unaltered. it's just another layer of
disablement, to absolutely ensure Intel ME is not alive

Signed-off-by: Leah Rowe <leah@libreboot.org>
---
 src/mainboard/dell/snb_ivb_latitude/cmos.default | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/src/mainboard/dell/snb_ivb_latitude/cmos.default b/src/mainboard/dell/snb_ivb_latitude/cmos.default
index 2a5b30f2b7..279415dfd1 100644
--- a/src/mainboard/dell/snb_ivb_latitude/cmos.default
+++ b/src/mainboard/dell/snb_ivb_latitude/cmos.default
@@ -6,4 +6,4 @@ bluetooth=Enable
 wwan=Enable
 wlan=Enable
 sata_mode=AHCI
-me_state=Normal
+me_state=Disabled
-- 
2.47.3

